Configuring motor on and off of motor on application

